|  | Great Game Database.com

Visit QuarterArcade
Browse Database
| Arcade Games
| Console Games
| Handheld
| Memorabilia
Technical Data:
| Arcade Manuals
| KB Articles
| Arcade Weights & Measurements
Collectors
| Online Collections
| Sign Up
| Log In
Special Thanks!
| Email Us : GreatGames@ QuarterArcade.com |
| Type > Arcade Games > Space Panic > KB-2687-191 |
Click here to return to viewing this item.
Overview
Name: | Space Panic
Year: | 1980
Genre: | Platform
Class: | Coin-Op
Sub-Class: | Arcade
Manufacturer: | Universal
Knowledge Base Article 2687-191
Title: Space Panic Pinout Author: spies.com Article:
    SPACE PANIC BOARD PINOUTS
    -------------------------
    (as typed in by Dr. Inferno, Jason Bardis, jasonbar@engineering.ucsb.edu,
     directly from the Space Panic manual, so, if these are wrong or make
     your Space Panic blow up, 'snot my fault.  I had both Video Connection's
     pinout sheet and the manual--they had a few discrepancies between the two
     and the manual's wiring diagram is less than elegant, but I think this
     is all okey-dokey.

    COMPONENT SIDE                         SOLDER SIDE
        GND                   1   A           GND
        GND                   2   B           GND
        +5V                   3   C           +5V
        +5V                   4   D           +5V
        +12V                  5   E           +12V
        -5V                   6   F           -5V
        GND                   7   H           GND
        +18V (audio thing?)   8   J           +18V (audio thing?)
        N/C (service?)        9   K           N/C
        COIN1 SLOT/COUNTER   10   L           AUDIO (line)
        1P CLOSing           11   M           N/C
        2P CLOSing           12   N           TILT
        1P UP                13   P           2P UP
        N/C                  14   R           N/C
        1P RIGHT             15   S           2P RIGHT
        N/C                  16   T           N/C
        1P DOWN              17   U           2P DOWN
        N/C                  18   V           N/C
        1P LEFT              19   W           2P LEFT
        N/C                  20   X           N/C
        1P START             21   Y           2P START
        1P HOLing            22   Z           VIDEO RED
        2P HOLing            23   a           VIDEO GREEN
        COIN2 COUNTER        24   b           VIDEO BLUE
        COIN2 SLOT           25   c           COMPOSITE SYNC (-)
        GND                  26   d           N/C
        GND                  27   e           GND
        N/C                  28   f           GND
Other Articles...
|  | KB-2687-191 Space Panic Pinout

Copyright © 2003, QuarterArcade.com, LLC